-------------------------------------------------------------------------------------------------------------
Latest information (2025.12.23)
-------------------------------------------------------------------------------------------------------------
The most recent versions of the TASCAM Sonicview Control are as follows.

Version: V2.3.1 (Previously V2.2.2 Updated at this time)

Note: Starting with application V2.3.1, the application is common to Sonicview 16/24 and Sonicview 16dp/24dp.

We request that you always use the latest version for TASCAM Sonicview Control.
For information about the latest version, check the TASCAM Global Site
 TASCAM Sonicview 16 / TASCAM Sonicview 16dp
   <https://tascam.jp/int/product/sonicview_16/support>
 TASCAM Sonicview 24 / TASCAM Sonicview 24dp
   <https://tascam.jp/int/product/sonicview_24/support>

-------------------------------------------------------------------------------------------------------------
Information about related equipment, software and other versions
-------------------------------------------------------------------------------------------------------------
The following information about versions is current as of December 23, 2025.
Please check individual product pages for the latest information.

- TASCAM Sonicview 16/16dp/24/24dp
　　- Firmware                         : V2.3.1    （date of latest update: 23 December 2025）

　　- Dante module firmware
      　< Brooklyn II >                            （date of latest update: 17 June 2025）
           Product Version             : V1.0.4   
           Software Version            : V1.0.4.2
           Firmware Version            : V1.0.4.2
           Dante Firmware Version      : V4.2.8.2

        < Brooklyn 3 >                             （date of latest update: 17 June 2025）
           Product Version             : V1.0.4
           Software Version            : V1.0.4.2
           Firmware Version            : V1.0.4.2
           Dante Firmware Version      : V4.2.9.4

- "TASCAM Sonicview Control" software for TASCAM Sonicview 16/16dp/24/24dp
  　- Version                          : V2.3.1    （date of latest update: 23 December 2025）

- "TASCAM Sonicview USB for Windows" USB driver for TASCAM Sonicview 16/16dp/24/24dp
    - Version                          : V1.10      (date of latest update: 1 April 2025)

- IF-MTR32 32-channel multitrack recording card for TASCAM Sonicview 16/16dp/24/24dp
　　- Firmware                         : V1.12     （date of latest update: 13 December 2023）

- SB-16D
    - Firmware                         : V1.21     （date of latest update: 1 April 2025）

　　- Dante module firmware
      　<TASCAM SB-16D units with serial numbers No.223xxxx, 226xxxx, 228xxxx（Brooklyn II）>    (date of latest update: 1 April 2025)
          Product Version              : V1.0.1
          Software Version             : V1.0.1.1
          Firmware Version             : V1.0.1.1
          Dante Firmware Version       : V4.2.8.2

        <TASCAM SB-16D units with serial numbers Serial No.232xxxx and later（Brooklyn 3）>     （date of latest update: 1 April 2025）
          Product Version              : V1.0.2
          Software Version             : V1.0.2.1
          Firmware Version             : V1.0.2.1
          Dante Firmware Version       : V4.2.9.4

- "TASCAM IO CONTROL" software for SB-16D
    - Version                          : V1.1.1     （date of latest update: 4 April 2024）

- IF-ST2110
    - Firmware                         : V0109      （date of latest update: 27 August 2025）

    - ST 2110 module                                （date of latest update: 27 August 2025）
          Firmware Version             ：V.2.1.16-j42
          FPGA Version                 ：V.1.0.0-b118
          WebUI Version                ：V.1.0.2-b026
<URLs>
 TASCAM Sonicview 16/16dp related :<https://tascam.jp/int/product/sonicview_16/support>
 TASCAM Sonicview 24/24dp related :<https://tascam.jp/int/product/sonicview_24/support>
 TASCAM IF-MTR32 related          :<https://tascam.jp/int/product/if-mtr32/support>
 TASCAM SB-16D related            :<https://tascam.jp/int/product/sb-16d/support>
 TASCAM IF-ST2110 related         :<https://tascam.jp/int/product/if-st2110/support>
=============================================================================================================

--------------------------------------------------------------------------------------------------------------
FW V2.3.1 (2025.12.23)
--------------------------------------------------------------------------------------------------------------
< New functions >
- New functions added in the main unit firmware (V2.3.1) are now supported.

< Maintenance items >
- When SB-16D was unmounted, sending commands such as Analog Gain changes via Ember+ could cause the application to terminate unexpectedly. This has been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V2.2.2 (2025.9.24)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- When the RTA function on the GEQ Screen was turned on, the RTA bar meters would not be displayed at the bottom of the MODULE (GEQ) Screen. This has been fixed.
- When “INPUT B” was selected as the input source for the ST IN1-2 modules, the input source on the Home Screen would sometimes not be correctly displayed. This has been fixed.

--------------------------------------------------------------------------------------------------------------
V2.2.1 (2025.7.10)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- When this app was newly installed on iPadOS 18, the Sonicview unit would sometimes not be detected because device search on the local network was turned off.
  This has been fixed so that a pop-up asking for permission to detect devices will now be displayed.
- On the Sonicview Control app HOME screen, the values shown in the ANALOG GAIN input fields for the SB-16D connected to the Sonicview unit would sometimes differ from the actual setting values. This has been fixed.

--------------------------------------------------------------------------------------------------------------
V2.2.0 (2025.6.17)
--------------------------------------------------------------------------------------------------------------
< New functions >
- New functions added in the main unit firmware (V2.2.0) are now supported.

< Maintenance items >
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V2.0.0 (2025.1.8)
--------------------------------------------------------------------------------------------------------------
< New functions >
- New functions added in the main unit firmware (V2.0.0) are now supported.

< Maintenance items >
- Maintenance items corrected in the main unit firmware (V2.0.0) are now supported.
- When a virtually mounted SB-16D input port was assigned to the input module, the PAD could not be turned on or off. This has been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V1.6.0 (2024.4.4)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- When performing copy/paste on the Compressor or Ducker with KEY IN SOURCE on "SELF" during remote connection, the main unit would not be set to "SELF". This has been fixed.
- During remote connection, changing the settings on the Custom Later SETUP screen on the main unit would not be reflected on the app. This has been fixed.
- During remote connection, changing the assignment of modules would result in the module meter not working properly. This has been fixed.
- During Offline Editor, the Mute button of a muted group or DCA would perform differently from that of the Sonicview unit. This has been fixed.
- After Factory Reset or All System Data Load, the Talkback setting would not switch to OFF. This has been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V1.5.1 (2023.11.14)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- Maintenance items corrected in the main unit firmware (V1.5.2) are now supported.

--------------------------------------------------------------------------------------------------------------
V1.5.0 (2023.10.18)
--------------------------------------------------------------------------------------------------------------
< New functions >
- New functions added in the main unit firmware (V1.5.0) are now supported.
- When remotely connected, saving from the Save Current Settings on the Sonicview Control app is now possible.

< Maintenance items >
- Issues with the Analog GAIN control not working properly when Analog input is selected for Insert Return have been fixed.
- Issues with MUTE settings not being properly reflected when recalling a Snapshot in Offline Editor mode have been fixed.
- The operation has been changed so that the selected FX RTN MUTE/SOLO is not turned ON or OFF even if the MUTE/SOLO of the MASTER section is operated when the SENDS ON FADER is turned on.
- GEQ numerical input issues have been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V1.4.0 (2023.7.26)
--------------------------------------------------------------------------------------------------------------
< New functions >
- User Key can now be operated when connected remotely.
- Libraries (EQ, Gate, COMP, GEQ, FX, and each module library) can now be operated when connected remotely.

< Maintenance items >
- When connected to the TASCAM Sonicview, controls from the application were sometimes not properly reflected in the Sonicview unit. This has been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V1.3.0 (2023.4.19)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- During remote connection, the Snapshot STORE/RECALL Confirmation settings of this software and the TASCAM Sonicview unit were not interlocked. This has been fixed.
- Operation stability has been improved.


--------------------------------------------------------------------------------------------------------------
V1.2.0 (2023.3.14)
--------------------------------------------------------------------------------------------------------------
< New functions >
- Linkage function with TASCAM IF-MTR32 is now supported.
- All System Data can now be saved and loaded in the desired location when in Offline Editor mode.
- New function (Ch mute/Pre-send link) added: the link operation of the input module Mute and the Pre Fader Send mute to the AUX bus can be set independently for each bus.

< Maintenance items >
- Control redundancy of TASCAM SB-16D is now supported.
　Notes: For this matter, users won’t be able to use the TASCAM SB-16D with FW V1.1.0
         In case of use in combination with the TASCAM SB-16D, please update this app and the TASCAM Sonicview unit up to firmware V1.2.0.
- POST COMP has been changed to PRE FADER in the Metering Point options for the CH1-40 module.
- Issues with the Copy Module in which Analog Gain, Pad, and HPF cannot be copied have been fixed.
- Issues in Module Library in which the STORE/RECALL function cannot be used with Library Module Input’s Analog Gain, Pad, and HPF have been fixed.
- The following issues with the Snapshot recall safe have been fixed:
　- In Parameter Safe, even when a checkmark was placed on the “Input/Osc parameters”, all Insert On/Off, Insert Point’s Recall Safe were validated. This has been fixed.
    From now on all Recall Safe functions will be validated after a checkmark is placed on “Insert Routing”.
  - In Parameter Safe, even when a checkmark was placed on “Effect Settings", Gate/Expander/Deesser parameters, Comp/Ducker parameters, and Delay parameters were validated. This has been fixed.
    From now on all Recall Safe functions will be validated after a checkmark is placed on "Other Module Parameters".
  - In Parameter Safe, even when a checkmark was placed on "Input Routing / Ch Stereo Link / Send Parameters" Pan/Bal’s Recall Safe was validated. This has been fixed.
    From now on all Recall Safe functions will be validated after a checkmark is placed on "Other Module Parameters",
  - In MODULE SAFE with the INPUT MODULE on ON, noise occurred on that INPUT MODULE when recalling SNAPSHOT. This has been fixed.
- When the ClockMaster is on Dante, changing the Sync Clock would trigger noise in Dante output. This has been fixed.
- Recall Snapshot would change the image in ST IN1 and ST IN2 to MONO. This has been fixed.
- Changing the INPUT MODULE’s PAD ON/OFF would change the Analog GAIN values and not match with the main unit. This has been fixed.
- In Stereo Link, this would be not displayed correctly or work properly. This has been fixed.
- The SOLO/MUTE indicator would not be displayed properly in the DCA module. This has been fixed.
- The DCA ASSIGN would not be displayed properly when recalling snapshots. This has been fixed.
- With MIX1-4, FX1-4 would not be displayed on the SENDS ON FADER screen when changing into SENDS ON FADER in the GROUP BUS mode. 
- When recalling/loading snapshots or All System Data, DCA-to-DCA assignments were not being properly recalled/loaded. This has been fixed.
- In the FX RTN module when recalling the MODULE Library, PRE/POST settings for the MIX1-22 and FX1-4 buses would turn to PRE settings when ALL SEND buses were displayed. This has been fixed. 
- The SENDS ON FADER of a grouped module in the BUS CONFIG tab would become controllable when the SENDS ON FADER screen is displayed. This has been fixed.
- The Paste module in MIX1-22 module (bus mode in AUX), or when Recall was performed in the MODULE Library, the MIX/FX SEND level indicator on the MODULE (OVERVIEW) screen would sometimes show the level to itself. This has been fixed.
- Sound would sometimes oscillate when performing Paste MODULE in the MIX1-22 module (bus mode in GROUP). This has been fixed.
- SENDS ON FADER operation could be performed for modules with bus mode set to GROUP in the BUS CONFIG tab of the MIXER CONFIG screen when the SENDS ON FADER screen was displayed. This has been fixed.
- Operation stability has been improved.


--------------------------------------------------------------------------------------------------------------
V1.1.1 (2022.12.14)
--------------------------------------------------------------------------------------------------------------
< Maintenance items >
- When a snapshot saved in OFFLINE EDITOR mode was recalled in OFFLINE EDITOR mode, custom layer settings would not be restored. This has been fixed.
- In V1.1.0, the device name would not be correctly saved in ALL SYSTEM DATA. This has been fixed.
- Operation stability has been improved.

--------------------------------------------------------------------------------------------------------------
V1.1.0 (2022.10.07)
--------------------------------------------------------------------------------------------------------------
< New functions >
- Support was added for linking with the TASCAM SB-16D.
- "INFORMATION" screen is available.
- "SOLO" bottun for each channel was added.

Note: Please refer to the Sonicview 16, Sonicview 24 Reference Manual for details on the new features.

< Maintenance items >
- Operation stability has been improved.
